Sea Trial  
  
Check bilges clean and dry before departure  
Ditto floor under engine and below stern lazarette  
Fold and unfold sprayhood  
Erect and stow cockpit tent  
Inflate dinghy  
  
Start engine and allow to warm up  
Switch on all instruments  
  
Cruising speed on engine 20 mins  
Check all instruments fully functional incl autopilot 10 mins  
Check heads fully functioning  
Check for engine leaks  
  
Fast cruise 5 mins  
Figure of eights forward and reverse  
Reverse 5 mins  
Check for engine leaks  
  
Set sails  
Sail on all points tacking and gybing 20 mins  
Fully furl and unfurl jib a few times  
Operate backstay tensioner  
Check all instruments fully functional incl autopilot 10 min  
  
Reef progressively  
Shake out reefs progressively  
Sail on all points when reefed tacking and gybing 10 mins  
Heave to

Anchor in 10 metres approx  
Drop and raise Jib and furl  
Test gas installation and make a cup of tea!  
Raise anchor  
  
Berth alongside  
Turn in own length  
Berth in normal marina berth  
  
Check for engine leaks  
Check bilges for leaks  
Check dinghy for leaks  
Check outboard functioning